**Commercial name**

**FreezeSafe Temperature Indicator**

**Company identification**

Authorized dealer: PROPAGROUP S.p.A.

Address: Via Genova, 5/B – 10098 RIVOLI (Turin) - Italy

www.propagroup.com - export@propagroup.com

Ph. +39 011 9507788 Fax +39 011 9507808

1. **Description and application**

FreezeSafe temperature indicators provide accurate evidence of a below threshold temperature excursion.

The FreezeSafe turns from clear to magenta when the temperature falls below its threshold. A visual check of the indicator alerts the recipient if the temperature has been unacceptably cold.

1. **Technical characteristics**

|  |
| --- |
| **Key Specifications** |
| Temperature Threshold | 0°C / 32°F2°C / 36°F |
| Time Delay | Within 90 minutes (2°C)Within 30 minutes (0°C) |
| Accuracy | ±1°C / ±2°F |
| Size | 21 x 21 mm |
| Visual Indication | Clear to Magenta |
| Storage Requirements | Store unused product away from direct lightbetween 15°C and 25°C / 59°F and 77°F |
| Shelf Life | 1 year |



**UNACTIVATED TRANSITION ZONE ACTIVATED**



**UNACTIVATED TRANSITION ZONE ACTIVATED**

1. **Production and Quality**

PROPAGROUP is UNI EN ISO9001 / ISO14001 certified and produces in accordance with the requirements of the main European and international standards in the sector.

The values indicated here are the result of standardised lab tests and meant only as an indication to help select and use the products. The user is responsible for ensuring the suitability and completeness of such information in relation to how the product is to be used.

**Written by:** Technical Management

**Revised by:** Quality Department

**Approved by:** Management